**HEAVY VEHICLE NATIONAL LAW**

**Victoria Class 3 Grain Harvest Management Scheme Mass Exemption Notice 2022 (No.1)**

1. Purpose

The purpose of this notice is to exempt a heavy vehicle to which it applies from stated prescribed mass requirements in Schedule 1 of the *Heavy Vehicle (Mass, Dimension and Loading) National Regulation* (the National Regulation) and operates in conjunction with the *Victorian Grain Harvest Management Scheme* (GHMS).

*Note: This Notice replaces the Victoria Class 3 Grain Harvest Management Scheme Mass Exemption Notice 2017 upon its expiry.*

1. Authorising Provision

This Notice is made under s117 of the Heavy Vehicle National Law (HVNL).

1. Title

This Notice may be cited as the *Victoria Class 3 Grain Harvest Management Scheme*

*Mass Exemption Notice 2022 (No.1).*

1. Commencement

The Notice commences on the 27 September 2022.

1. Expiry

This Notice expires on 26 September 2027.

1. Definitions
2. Unless otherwise stated, words and expressions used in this notice have the same meanings as those defined in the *Heavy Vehicle National Law*.
3. In this Notice:-

***Eligible Vehicle*** means a vehicle that meets the description of a combination under column 1 of Table 1: Conditional Mass Limits under section 11 of this Notice.

***Grain*** means a grain specified in the Scheme

***Participating Grain Receiver*** means a facility that is registered as a participating receiver under the Scheme by way of a signed Participating Grain Receiver Undertaking and Signature Form lodged with Department of Transport.

***Victoria Grain Harvest Management Scheme*** (the Scheme) means the scheme of that name maintained and administered by Department of Transport as described in the “*Victorian Grain Harvest Management Scheme – Operating Guidelines*.”

***Department of Transport*** means the Victorian state Road Authority called The Roads Corporation.

1. Application

This Notice applies to an eligible vehicle operating in Victoria that are transporting grain from the place where the grain was loaded to a participating grain receiver and that meets all of the requirements of this Notice.

1. Exemption from Prescribed Mass Requirements
2. This notice exempts a vehicle to which it applies from the following general mass limits specified in Schedule 1 of the *National Regulation*:
3. Section 2(1)(a)(iv);
4. Section 2(1)(b);
5. Section 2(2);
6. Section 2(4);
7. Section 4;
8. Section 5(1) and (2); and
9. Part 2, Table 1, 2 & 3.
10. Areas or routes
11. A heavy vehicle operating under this notice may operate on one of the following stated networks maintained by Department of Transport;
12. for Rigid and Semi-trailers; *Grain Harvest Management Scheme Rigid Truck & Semi-Trailer Network.*
13. for B-Doubles; *Grain Harvest Management Scheme B-double Network.*

*Note: online maps for these networks are maintained on the* Department of Transport *website.*

1. Conditions – Vehicle Standards and Registration
2. An eligible vehicle operating under this notice must comply with the following requirements:
3. have been manufactured on or after 1 January 2002; and
4. comply with Vehicle Standard (Australian Design Rule 80/00 - Emission Control for Heavy Vehicles) 2005.
5. Conditions – Mass Limits
6. The maximum loaded mass of a heavy vehicle must not exceed the lowest of the following:
7. In the case of a combination, the GCM limit specified by the prime mover manufacturer; or
8. In the case of a combination, the sum of the GVMs for the prime mover and the trailer or trailers it is towing; or
9. In the case of a truck, the GVM of the vehicle; or
10. The mass limit for the heavy vehicle set out in Table 1 of this Notice.

**Table 1: Conditional Mass Limits**

|  |  |
| --- | --- |
| **Column 1** | **Column 2** |
| **VEHICLE OR COMBINATION** | **MASS LIMIT**  **(Tonnes)** |
| Single steer, single drive rigid truck | 16.8 |
| Single steer, tandem drive rigid truck | 23.6 |
| Twin steer, tandem drive rigid truck | 28.9 |
| Single steer, single drive prime mover and single axle semitrailer | 27.3 |
| Single steer, single drive prime mover and tandem axle semitrailer | 34.1 |
| Single steer, single drive prime mover and triaxle semitrailer | 37.8 |
| Single steer, tandem drive prime mover and tandem axle semitrailer | 41.0 |
| Single steer, tandem drive prime mover and triaxle semitrailer | 44.6 |
| Single steer, tandem drive rigid truck and 2 axle dog trailer | 42.5 |
| Single steer, tandem drive rigid truck and 4 axle (tandem – tandem) dog trailer | 44.6 |
| B-double (up to 19m) (General access vehicle) - Single steer, tandem drive prime mover towing two tandem axle semitrailers | 52.5 |
| B-double (up to 19m) (Restricted access vehicle) - Single steer, tandem drive prime mover and tandem axle semitrailers | 58.3 |
| 25/26m B-double (Restricted access vehicle) - Single steer, tandem drive prime mover towing two triaxle semitrailers | 65.6 |

1. Steer axle mass exception (total mass limit) condition

A heavy vehicle that complies with the requirements of Schedule 3 of the *National Regulation* (Steer axle mass exception limits) may exceed the mass limit in Table 1 by 0.5 tonnes.

Peter Caprioli

*Executive Director Access*

**National Heavy Vehicle Regulator**