HEAVY VEHICLE NATIONAL LAW

New South Wales Class 3 Port Botany Container Transportation Mass Exemption Notice 2024 (No.1)

1. Purpose

1) This notice grants exemptions from mass requirements for certain configurations of eligible class 3 heavy vehicles transporting over-mass freight containers from a Stevedore’s Terminal at Port Botany to a prescribed Container Freight Station.

Note: This notice operates in conjunction with the New South Wales Class 2 and 3 Port Botany Container Transportation Mass Exemption Notice Operator’s Guide.

1. Authorising Provision

1) This notice is made under the following section of the Heavy Vehicle National Law (HVNL):

a) section 117 – *Regulator’s power to exempt category of class 1 or 3 heavy vehicles from compliance with mass or dimension requirement*.

1. Title

This notice may be cited as the *New South Wales Class 3 Port Botany Container Transportation Mass Exemption Notice 2024 (No.1).*

1. Commencement

This notice commences on 11 June 2024.

1. Expiry

This notice expires on 10 April 2029.

1. Definitions
2. Unless otherwise stated, words and expressions used in this notice have the same meanings as those in the HVNL and its regulations.
3. In this notice:

***Container Freight Station (CFS)*** means a CFS prescribed in the Guide.

***Guide*** meansthe *New South Wales Class 2 and 3 Port Botany Container Transportation Mass Exemption Notice Operator’s Guide* published by the National Heavy Vehicle Regulator, as amended from time to time.

***MDL Regulation*** means the *Heavy Vehicle National (Mass, Dimension and Loading) Regulation.*

***Prescribed Stevedore’s Terminal*** means a cargo terminal prescribed in the Guide.

1. Application
2. This notice applies to a class 3 heavy vehicle that meets all the requirements in this section.
3. This notice applies to a vehicle that is one of the following categories, and that is carrying a load of one or more freight containers from a Prescribed Stevedore’s Terminal:
4. a rigid truck;
5. a prime mover and semi-trailer combination that has an overall length not exceeding 19 metres, and not more than 6 axles in total;
6. a B-double that has an overall length not exceeding:
	* 1. 19 metres, and not more than 7 axles in total; or
		2. 23 metres, and not more than 8 axles in total; or
		3. 26 metres, and 9 axles in total.
7. A vehicle to which this section applies and that complies with the conditions of this notice is an eligible vehicle.
8. Exemption – Prescribed Mass Requirements

1) An eligible vehicle is exempt from the following mass requirements under Schedule 1 of the MDL Regulation:

a) section 2 – Mass limits for a single vehicle or combination

b) section 4 – Mass limits for a single axle or axle group

c) section 5 – Mass limits relating to axle spacing generally

2) An exemption in 1) applies to an eligible vehicle only to the extent that specific conditional mass limits are provided in section 9 of this notice.

3) Regardless of any conditional masses prescribed in this notice an eligible vehicle must not exceed manufacturer mass limits as defined in section 8 of the MDL Regulation.

1. Conditions - Mass Limits

An eligible vehicle operating under this notice must not exceed the mass limits specified in Table 1.

**Table 1 Axle mass limits**

|  |  |
| --- | --- |
| **Description** | **Maximum Allowable Mass (t)** |
| A non-complying steer axle | 7.2 |
| A complying steer axle  | 7.8 |
| Single axle or single axle group fitted with single tyres with section widths of at least 375mm | 7.8 |
| Single axle or single axle group fitted with single tyres with section widths of at least 375mm but less than 450mm | 8.04 |
| Single axle or single axle group fitted with single tyres with section widths of at least 450mm | 8.40 |
| Single axle or single axle group fitted with dual tyres on a vehicle that is not a pig trailer, complying bus or ultra-low-floor bus | 10.8 |
| Tandem axle group fitted with single tyres with tyre section widths of less than 375mm | 13.2 |
| Tandem axle group fitted with single tyres with tyre section widths of at least 375mm but less than 450mm | 15.96 |
| Tandem axle group fitted with single tyres with tyre section widths of at least 450mm | 16.8 |
| Tandem axle group fitted with single tyres on 1 axle and dual tyres on the other axle on a motor vehicle that is not a complying bus  | 15.6 |
| Tandem axle group fitted with dual tyres on a vehicle that is not a pig trailer | 19.8 |
| Twinsteer axle group without a load-sharing suspension system | 12.0 |
| Twinsteer axle group with a load-sharing suspension system.  | 13.2 |
| Tri-axle group on a vehicle other than a pig trailer fitted with -1. single tyres with section widths of at least 375mm on all axles
2. dual tyres on all axles
3. single tyres with section widths of at least 375mm on some axles and dual tyres on the other axles
 | 24.0 |
| Quad-axle group fitted with single tyres with section widths of less than 375mm | 18.0 |
| Quad-axle group fitted with single tyres with section widths of at least 375mm or dual tyres | 24.0 |

**10. Condition – stated areas or routes**

1. An eligible vehicle complying with the conditions of this notice is authorised to operate on areas and routes stated in this section.
2. For the purposes of section 119 (1)(a) of the HVNL, an area or route stated in this section is a stated area or route to which this notice applies.
3. An eligible vehicle may operate on the areas and routes as listed in ‘*Schedule 1 – Approved Routes and Condition*’ of the Guide.
4. Regardless of any access granted under this section, an eligible vehicle must comply with any conditions or restrictions applied to a given area or route by the *Specified Road Manager Network Requirements* in the Guide.
5. In this section:

***Network*** means a map or stated route, including a list or database, presented electronically or otherwise, that represents the stated areas and stated routes authorised under this notice.

1. An eligible vehicle operating on an area or route specified in a schedule must comply with any of the following conditions prescribed for that area or route:
2. Road conditions pursuant to section 160 of the HVNL; and
3. Travel conditions pursuant to section 161 of the HVNL; and
4. Vehicle conditions pursuant to section 162 of the HVNL.

Peter Austin

*Director Policy Implementation*

**National Heavy Vehicle Regulator**