

**1900–1920 MHz Frequency Band Plan 2012**

The AUSTRALIAN COMMUNICATIONS AND MEDIA AUTHORITY makes this Frequency Band Plan under sections 32 and 34 of the *Radiocommunications Act 1992*.

Dated *26 March* 2012

*Chris Chapman*
[signed]
Member

*Richard Bean*
[signed]
 ~~General Manager~~/Member

Australian Communications and Media Authority

**Contents**

1 Name of Frequency Band Plan 2

2 Commencement 2

3 Revocation 2

4 Interpretation 2

5 Purpose of Frequency Band Plan 3

6 Purposes for which the 1900–1920 MHz frequency band may be used 3

**1 Name of Frequency Band Plan**

 This Frequency Band Plan is the *1900*–*1920 MHz Frequency Band Plan 2012.*

**2 Commencement**

 This Frequency Band Plan commences on the day after it is registered.

*Note* All legislative instruments and compilations are registered on the Federal Register of Legislative Instruments kept under the *Legislative Instruments Act 2003.* See http://www.frli.gov.au.

**3 Revocation**

 The *1900*–*1920 MHz and 2010*–*2025 MHz Bands Frequency Band Plan 2004* is revoked.

**4 Interpretation**

 (1) In this Frequency Band Plan:

***Act*** means the *Radiocommunications Act 1992*.

***interpretation determination*** means the *Radiocommunications (Interpretation) Determination 2000*.

***point-to-multipoint*** means transmissions between a specified fixed station and two or more associated fixed stations.

***point-to-point*** means transmissions between two specified fixed stations.

***primary service*** has the same meaning as in Part 1 of the spectrum plan.

***regulations*** means the *Radiocommunications Regulations 1993*.

***secondary service*** has the same meaning as in Part 1 of the spectrum plan.

***spectrum plan*** means the *Australian Radiofrequency Spectrum Plan* *2009*.

 (2) Unless the contrary intention appears, an expression used in this Frequency Band Plan that is defined in the spectrum plan, the interpretation determination or the regulations has the same meaning in this Frequency Band Plan as it has in the spectrum plan, the interpretation determination or the regulations.

 (3) However:

 (a) an expression defined in the spectrum plan and in the interpretation determination or the regulations has the meaning given in the spectrum plan; and

 (b) an expression defined in the interpretation determination and in the regulations (but not in the spectrum plan) has the meaning given in the interpretation determination.

*Note*The following expressions used in this Frequency Band Plan are defined in the spectrum plan:

• fixed service

• mobile service.

 (4) In this Frequency Band Plan, the range of numbers that identifies a frequency band is taken to include the higher, but not the lower, number.

*Example*

The 1900–1920 MHz frequency band is made up of radio frequencies that exceed 1900 MHz but do not exceed 1920 MHz.

**5 Purpose of Frequency Band Plan**

 This Frequency Band Plan makes provision for the purposes for which the 1900–1920 MHz frequency band may be used.

**6 Purposes for which the 1900–1920 MHz frequency band may be used**

 The 1900–1920 MHz frequency band may be used for the following primary services and secondary services:

|  |  |
| --- | --- |
| Primary Services | Fixed Service(point-to-multipoint)Mobile Service |
| Secondary Service | Fixed Service(point-to-point) |