**HEAVY VEHICLE NATIONAL LAW**

**New South Wales Class 3 Livestock Transportation Exemption Notice 2021 (No.1)**

1. **Purpose**
2. This Notice provides mass exemptions that support the New South Wales Livestock Loading Scheme. This Notice works with the New South Wales Livestock Loading Scheme, and gives effect to the exemptions and conditions of that Scheme. Compliance with the Scheme is a condition of this Notice.
3. This Notice revokes and replaces the *New South Wales Class 3 Livestock Transportation Exemption Notice 2020 (No.1)*.

*Note: The New South Wales Livestock Loading Scheme is published and maintained by Transport for New South Wales (TfNSW), in conjunction with the National Heavy Vehicle Regulator (NHVR).*

*This version of the Notice includes access to the New South Wales Farm Gate Network.*

1. **Authorising Provision**

This Notice is made under section 117 of the *Heavy Vehicle National Law*.

1. **Title**

This Notice may be cited as the *New South Wales Class 3 Livestock Transportation Exemption Notice 2020 (No.2)*.

1. **Commencement**

This notice commences on 26 February 2021.

1. **Expiry**

This notice expires on 9 February 2024.

1. **Application**

This notice applies to eligible combinations operating in New South Wales.

1. **Definition**
2. Unless otherwise stated, words and expressions used in this notice have the same meanings as those defined in the HVNL.
3. In this Notice:

**Combined loading space** means the sum of the loading spaces of each vehicle that is part of an eligible combination.

**Eligible combination** means a heavy vehicle combination that is eligible to operate under this Notice as specified in s8.

**General Access** means access to all roads in New South Wales, subject to the New South Wales Road Rules and the HVNL.

**Loading space** means the dimension measured from the inside of the front wall or door to the inside of the rear wall or door of a semi-trailer, with intervening partitions being disregarded.

**Scheme** means the New South Wales Livestock Loading Scheme published and maintained by TfNSW.

1. **Eligible combinations**
2. An eligible combination must be one of the following category of heavy vehicle:
3. Single articulated vehicles which consist of a prime mover and a semi-trailer, and have a loading space available for the carriage of animals not exceeding 12.5 metres;
4. B-doubles that have an overall length not exceeding 19.0 metres and a combined loading space available for the carriage of animals not exceeding 15.0 metres; and
5. B-doubles that have an overall length not exceeding 26.0 metres and a combined loading space available for the carriage of animals not exceeding 18.8 metres; and
6. Road trains that have an overall length not exceeding 36.5 metres, and a minimum distance between the centres of the outermost axles of a road train of at least 26.5m metres, and a combined loading space available for the carriage of animals not exceeding 25.0 metres.
7. B-triples that consist of a prime mover and three semi-trailers and have a combined loading space available for the carriage of animals not exceeding 28.2 metres.
8. AB-triples that consist of a prime mover and semi-trailer combination connected, by a converter dolly, to two semi-trailers which are connected by a fifth wheel coupling, that have a combined loading space available for the carriage of animals not exceeding 28.2 metres.
9. A vehicle under this section is only an eligible combination when it is transporting livestock.
10. **Conditions - Vehicle Requirements**
11. Eligible combinations operating under this notice must have:
12. a prime mover with a tandem axle drive group, and
13. semi-trailer(s) with either tandem axle or tri-axle group(s), or in the case of a B-double not exceeding 19.0 metres in length, semi-trailers with tandem axle groups only; and
14. in the case of a road train or an AB-triple, either a tandem axle or tri-axle group on the converter dolly, and
15. either single tyres with section width of at least 375 mm, dual tyres, or a combination of those tyres, on all axle groups, and
16. certified road friendly suspension fitted and maintained in working order on all axle groups of all semi-trailers.
17. in the case of a B-Triple or AB-triple, certified road friendly suspension fitted and maintained in working order on all axle groups.
18. **Exemption – Mass**
19. Eligible combinations operating under this Notice are exempt from the following mass requirements in Schedule 1 of the *Heavy Vehicle (Mass, Dimension & Loading) National Regulation (MDL Regulation)*:
20. section 2(1)(a)(iv) - Complying steer axles for vehicles that are not B-Doubles or Road Trains.
21. section 2(1)(2(b) - Axle Mass limits referencing Table 1, Part 2.
22. section 4 and Table - Mass limits for a single axle or axle group.
23. section 5 - Mass Limits relating to axle spacing generally.
24. These exemptions only apply to a mass requirement where a conditional mass for a specified parameter has been provided in this Notice.
25. **Conditions - Mass (Gross Combination Mass)**
26. The total mass of a combination must not exceed the lowest of the following:
27. the sum of the axle and axle group mass limits in Table 1, or
28. the GCM limit specified by the prime mover manufacturer, or
29. the sum of the GVMs for the prime mover and the trailer or trailers it is towing.
30. **Conditions - Mass (Axle and axle group limits)**
31. The mass on an axle or axle group must not exceed the limits set out in Table 1, except as provided for by 2).

**Table 1: Axle and axle group mass limits**

|  |  |
| --- | --- |
| **STEER AXLE GROUPS** | **MASS LIMIT (t)** |
| Single steer axle | 6.0 |
| **NON-STEER AXLE GROUPS** |  |
| Tandem axle group not fitted with certified road friendly suspension | 16.5 |
| Tandem axle group fitted certified road friendly suspension | 17.0 |
| Tri-axle group not fitted with certified road friendly suspension (converter dollies only) | 16.5 |
| Tri-axle group fitted with certified road friendly suspension | 22.5 |

1. Floating tri-axle mass concession: the mass on a tri-axle group of a semitrailer may exceed the limit set out in Table 1 by up to 0.5 tonne, as long as the total mass of the combination does not exceed the total mass limit (GCM) specified in section 11.
2. **Conditions – Stated Areas and Routes**
3. An eligible combination operating under this Notice may operate access the following network
4. Eligible single articulated vehicles up to 19.0 metres in length:

*New South Wales Livestock Loading Scheme Single Articulated Combination Network*

1. Eligible B-doubles up to 19.0 metres in length:

*New South Wales Livestock Loading Scheme 19m B-double Network*

1. Eligible B-doubles up to 23.0 metres in length:

*New South Wales Livestock Loading Scheme 23m B-double Network*

1. Eligible B-doubles up to 26.0 metres in length:

*New South Wales Livestock Loading Scheme 26m B-double Network*

1. Eligible Type 1 A-double road trains up to 36.5 metres in length:

*New South Wales Livestock Loading Scheme Type 1 A-double Network*

1. Eligible B-triple road trains up to 36.5 metres in length:

*New South Wales Livestock Loading Scheme B-triple Network*

1. Eligible AB-triple road trains up to 36.5 metres in length:

*New South Wales Livestock Loading Scheme AB-triple Network*

1. An eligible vehicle accessing a network set out in subsection (1) must comply with the road and travel conditions set out in that network.

*Note: Links and descriptions of these routes may be found in the Scheme Business Rules.*

1. An eligible vehicle accessing a network set out in subsection (1) may also access the *New South Wales Farm Gate Network* if it is enrolled in the *Road Infrastructure Management (RIM)* approved intelligent transport system pursuant to s14(3) of this Notice.

*Note:- The New South Wales Farm Gate Network is published on the New South Wales Farm Gate Network webpage, published on the TfNSW website. This network includes networks in participating Road Manager areas, including the travel and road conditions that apply on those networks.*

*Note:- Access to the networks under this section may require that the eligible vehicle be enrolled in and comply with an approved intelligent transport system pursuant to s14 of this Notice.*

1. **Conditions - Intelligent Access Conditions**
2. B-triples and AB-triples may only operate under this Notice if they are enrolled in one of the following approved intelligent access system pursuant to Chapter 7 of the HVNL:
3. The Telematics Monitoring Application (TMA) with Transport Certification Australia (TCA); or
4. The Intelligent Access Program (IAP) with TfNSW.
5. B-triples and AB-triples operating under (1)(b) must comply with all of the conditions relating to IAP in s10 of the *New South Wales Higher Mass Limits Declaration 2020.*
6. An eligible vehicle operating on the *New South Wales Farm Gate Network* must be enrolled in the Road Infrastructure Management (RIM) approved intelligent access system pursuant to Chapter 7 of the HVNL.

*Note:- Approved intelligent transport systems are developed by Transport Certification Australia (TCA) under the National Telematics Framework. Information on the Framework and approved intelligent transport systems may be found on the TCA website.*

1. **Conditions- New South Wales Livestock Loading Scheme**
2. An eligible combination operating under this notice must comply with all of the requirements of the New South Wales Livestock Loading Scheme, including but not limited to:
3. Eligible livestock; or
4. Deck requirements; or
5. Driver accreditation; or
6. Registration; or
7. Interstate mutual recognition requirements; or
8. conditions relating to routes as per the networks specified in s14.

Peter Caprioli

*Executive Director (Freight and Supply Chain Productivity)*

**National Heavy Vehicle Regulator**